G+ Mass Production Tool Ver 2.1.2 - Mar. 18, 2015
==============================================================================
- Support readback verify function.
- Support multi-device operation.
- Add log message for each USB command.
- Support a maximum of 100 pre-register sets.
- Add NVRAM type to support SPIFC mode.

G+ Mass Production Tool Ver 2.1.1 - Jan 28, 2011
==============================================================================
- Modified dialog message box displaying.
- Modified the rule of checking SW tool version.
- Modified DelayPC Action to DelayStep.
- Modified Pre-register value when device number was changed.
- Modified Code Path opening method when user click ... button.
- Updated 8k page Nand driver conf file.
- Modidy template script file for verify option.
- Add read back verify & check sum verify option enable or disable issue.
- Modified std template script file to disable erase all block step.
- Added step rename function.
- Modified residue sectors to total sectors.
- Add residue sector size(4Bytes) when send write command to device.
- Modify check sum verification calculation.
- Add check sum verification mode when usb boot bin was changed dynamically.
- Modify user defined command format.

G+ Mass Production Tool Ver 2.1.0 - Oct 27, 2010
==============================================================================
- Add disable setting button function when exported by Codepacker.
- Add LRunas Dll to promote the authorization of User.
- Add Probe path function with new ICE Driver to support GP5(just single 
- device at present.)
- Add readback verify fucntion for writing serial number step.
- Modify UI layout and alignment issue.
- Modified user customerized read command parameters format.
- Fixed Compare function between two files.
- Fixed plents of memory leaks when downloading with multi-device.
- Fixed readback verify fail issue when writing serial number to MLC Flash.
- Fixed issues : compare file failure even two files are same.
- Fixed UI showing issue when up or down compare file step.
- Fixed crash issue when click browse button with compare file step.
- Removed GetNandInfo & CheckBadBlkRate function when write boot area.

USB Mass Tool Ver 2.0.9 - June 25, 2010
==============================================================================
- Modified to enhance delete function of bin & zip files after downloading,
  include encountered reset or power off when downloading.
- Add delete function of bin & zip files after downloading, if it has hdb file
- Modified the showing methods if the directory was created failure.
- Removed the package version showing if autoerase option was checked.
- Fixed Crash problem when user have no authorization to access file  .
- Rename USBMassProductionTool to G+MassProductionTool.
- Update GPMPPack Bin Library for new hdb files.
- Modified SW Tool Version verification from 4 to 3 section
- Fixed boot script file switching failure when power on again.
- Modify Step retry mechanism if one step failure and specific retry count.
- Modify File filter for file selecting.
- Modify HDB files Version information display function, replaced by static 
- text and removed previous check box selecting .
- Modify version showing sequency and alignmant.
- Removed space between characters and version numbers.
- Add HDB files Version information display function.
- Add HDB files verify machanism, including sw tool id , sw tool version, body
  name and so on.

USB Mass Tool  Ver 2.0.8 - May 04, 2010
===============================================================================
- Add get version number from resource view function.
- Modified Progress bar color display.
- Update CPU name according to formal naming rule.
- Modify pre-reister dialog setting when select different numbers.
- Modify 0x2A2A command when it works on vista.
- Modify UI display if select autowrite app or date area.
- Added Delay time before read back verify function when write date each time.
- Added Step retry mechanism if each step failed.
- Fixed bug: It does not need to check the boot bin file name.
- Fixed Pre-register setting failure when called by codepacker.
- Fixed Send pre register cmd when register number is zero.
- Fixed bug: Does not need to check BCH bin file name.
- Fixed bug: Pre-register max text length limitation.

USB Mass Tool  Ver 2.0.6 - Jan 07, 2010
===============================================================================
- Add Write Serial Number request.
- Modify disable step check control function when it is checked.


USB Mass Tool  Ver 2.0.5.3 - Dec 3th, 2009
===============================================================================
- Add parser library for boot script file and usbtools ini file.
- Modify the GUI to apply to changed request for UI, and worked independently.
- Modified the version to 2.0.5.3

USB Mass Tool  Ver 2.0.5.2 - Nov 17th, 2009
===============================================================================
- Added re-enumerate function when user select new sccript file and enumerate 
- 			devices with the cup type in script file.
- Modified message dialog when no device be enumerated in download or enumerate.
- Fixed bug that does not download at the time with more than one devices.
- Modified the version to 2.0.5.2

USB Mass Tool  Ver 2.0.5.1 - Nov 09th, 2009
===============================================================================
- Added message dialog when no device be enumerated.
- Removed the version number in usbtools.ini file.
- Removed the cpu selection dialog whatever called coder packer.
- Modified the version to 2.0.5.1

USB Mass Tool  Ver 2.0.5 - Nov 6th, 2009
===============================================================================
- Modified version 2.0.4.4 to V2.0.5 .

USB Mass Tool  Ver 2.0.4.4 - Nov 6th, 2009
===============================================================================
- Fixed bug: read App Area size from downloadinfo.ini file when write SPI Flash.
-            without codepacker.

USB Mass Tool  Ver 2.0.4.3 - Nov 6th, 2009
===============================================================================
- Fixed bug: read App Area size from downloadinfo.ini file when write SPI Flash.

USB Mass Tool  Ver 2.0.4.2 - Nov 5th, 2009
===============================================================================
- Add report information if the size of App bin file or RWImage file is zero.
- Modified AutoDownloadNand config file step .
- Updated FW Nand bin file in code folder.
- Fixed bug: could not download when the size of RWImage file is zero.
- Fixed bug: occur runtime error when download spi in release version.

USB Mass Tool  Ver 2.0.4.1 - Nov 4th, 2009
===============================================================================
- remove the CPU Setting Dialog when called by code packer.

USB Mass Tool  Ver 2.0.4 - Oct 12th, 2009
===============================================================================
- Add auto write boot area and app area function with codepacker.
- Add Pre-register function with codepacker.
- Add GPlusUSBDownload Lib API Specification.
- Fixed WndCUI version resource release issue caused exception when download twice
- or more time with different config file.

USB Mass Tool  Ver 2.0.3 - August 12th, 2009
===============================================================================
- Fixed bug of GetChipType function for Mac OS Version.

USB Mass Tool  Ver 2.0.2.5 - August 7th, 2009
===============================================================================
-	Add test config file for 16 and 32 bit.
- Add pid & vid to support GP11 in ini file. default is empty.
- fixed a bug that send command 0xff44 failure for Mac version

USB Mass Tool  Ver 2.0.2.4 - July 20th, 2009
===============================================================================
- Add function that read back verify failure ,the program will be go on executing.
- Modify usbtool.ini file, to add identifier to distinguish on or off.
- Modify 16 bit read back veriry status.

USB Mass Tool  Ver 2.0.2.3 - June 12th, 2009
===============================================================================
- Add function that do not read back verify when it found bad block.
- Add 0xFF48 Cmd to get the bad block info, including bad block number and size.
- Add 'break' insturction to get the correct error code of sense key.
- Modify to report some bad block info in log when each step finished.

USB Mass Tool  Ver 2.0.2.2 - April 30th, 2009
===============================================================================
- Add Erase All NandFlash blocks function;
- Add Power on and Power off function for OTP in GP4(162004).

USB Mass Tool  Ver 2.0.2.1 - April 30th, 2009
===============================================================================
- Add Get Nand ID 0xff45 interface in GPL32FlashIO class, for VTech. provide by 
- xh in 1 department

USB Mass Tool  Ver 2.0.2 - April 8th, 2009
===============================================================================
- Add Boot write to handle bad block
- Add Nand OTP to support GP4 Nand OTP R/W.
- Add select cpu dialog to identify the usb device automatically.
- Add Create File automatically according to the user specified when read.
- Modify some Unit display in UI.
- Modify the data length have not save normally.
- Fix a bug when send 0xFD2A command failure.
- Del BCH Count Setting in the Boot Write Dialog.

GPLXXX Mass Tool  Ver 2.0.0.3 - March 12th,2009
=================================================================================
- Add Open button in USBToolDlg, 
- Add a funtion when readback verify was checked. save a file to disk.
- Add Unit for address(Byte) and length(Block)  
- Add USB Command 0xFF40 as SetAppVariable.
- Modify Jump to Funtion command: only remain RAM Option.
- Modify nand flash to SLC nand to distinguish 
- Remove option of "write with auto erase" in Write step.
- Fixed a bug when disable write command,it will also request to select code file.
- Fixed a bug when change cpu type betweent 16 and 32 with open bootscript.

GPLXXX Mass Tool Ver 2.0.0.2 - March 2th, 2009
=================================================================================
- add data lentth option when read/write
- add time-out option when download 

GPLXXX Mass Tool Ver 2.0.0.1 - Feb 20th, 2009
=================================================================================
 - combine the GPL162002&162004 and GPL32xxx Mass Tool.

MassProductionTool_162002_162004 Ver 1.0.3.8 - Jan 13th, 2009
=================================================================================
 - fix two bug: relative path and the limit of the file length 128 byte.
 - Modify User Command:
	a) Write can do not specify the file.
	b) Write: if specify the file, the specified format in the remard will 
	          be as follow:
	CMD1	CMD0	Addr3	Addr2	Addr1	Addr0	Rev	Len1	Len0
	c) Read: if specify to read the file , you need to point a end address. 
                 the format in the reamark will be as follow:
	CMD1	CMD0	Addr3	Addr2	Addr1	Addr0	Rev	Len1	Len0	
 - compare two file whether right or wrong individually. 


MassProductionTool_162002_162004 Ver 1.0.3.7 - Dec 29th, 2008
=================================================================================
 - Add a Error code named  SenseKey_Original_Bad_Block, when R/W error and return 
   error according huck's request.

MassProductionTool_162002_162004 Ver 1.0.3.6 - Dec 24th, 2008
=================================================================================
 - Add Auto Ready function after device download completely according the request 
   of sixthDepartment 

MassProductionTool_162002_162004 Ver 1.0.3.5 - Dec 8th, 2008
=================================================================================
 - Modify the response speed for ChipErase command from 2 minustes to 10 minutes.

MassProductionTool_162002_162004 Ver 1.0.3.4 - Novem 11th, 2008
=================================================================================
 - Add Action type for App Area Format and Initial step
 - cmd is as below£º 
 - CMD FF34  APPFormat 
 -          parameters£º  0x10  Erase expect user mark 
 -                        0x01  ALL Erase   
 - CMD FF35  APPInit

MassProductionTool_162002_162004 Ver 1.0.3.3 - Novem 7th, 2008
=================================================================================
 - Add the parameter function for SendCommand.
 
MassProductionTool_162002_162004 Ver 1.0.3.2 - Novem 5th, 2008 ================================================================================
 - Add the support of MLC 2k + 64byte(Physical)
 
MassProductionTool_162002_162004 Ver 1.0.3.1 - Oct 24th, 2008
=================================================================================
 - Modify the read address of writing certification as write address. the old 
   version is placed the fixed address 0x30000.

MassProductionTool_162002_162004 Ver 1.0.3.0 - June 19th, 2008
=================================================================================
 - Add button enuming device manually
 - Add lock operation for SetNoMount function.
 - Modify the DeviceIoControl in GPlusUSBLib library.
 - fixed a problem that enumerate device frequently when haven't plugged devices.

MassProductionTool_162002_162004 Ver 1.0.2.12 - June 18th, 2008
=================================================================================
 - we should use RegisterDeviceNotification function, this is because it will 
   trigger the DBT_DEVICEARRIVAL event when calling SetNoMount function.

MassProductionTool_162002_162004 Ver 1.0.2.11 - June 17th, 2008
=================================================================================
 - it will occur plenty of WM_DEVICECHANGE message when the devices will be 
   plugged in or out so it have been fixed in this version.

MassProductionTool_162002_162004 Ver 1.0.2.10 - May 28th, 2008
=================================================================================
 - Add Auto Test download function.

MassProductionTool_162002_162004 Ver 1.0.2.9 - May 23th, 2008
=================================================================================
 - remove ReadICVersion function because it is reported occur problem frequently 
   by customer when executing ReadIC Version function. Huck's decision

MassProductionTool_162002_162004 Ver 1.0.2.8  May 19th, 2008
=================================================================================
  - list the error sector number in wrong information just as read compare command.

Ver 1.0.0.0  
 - 