C51 COMPILER V9.52.0.0   GPIOINIT                                                          09/28/2018 11:21:01 PAGE 1   


C51 COMPILER V9.52.0.0, COMPILATION OF MODULE GPIOINIT
OBJECT MODULE PLACED IN .\Output\GPIOInit.obj
COMPILER INVOKED BY: D:\FortiorTech\Software\Mcu\C51\BIN\C51.EXE ..\User\Source\Hardware\GPIOInit.c LARGE OMF2 WARNINGLE
                    -VEL(0) BROWSE INCDIR(..\Library\FU68xx_Hardware_Driver\Include;..\User\Include) DEBUG PRINT(.\Listing\GPIOInit.lst) OBJE
                    -CT(.\Output\GPIOInit.obj)

line level    source

   1          /**************************** (C) COPYRIGHT 2017 Fortiortech shenzhen *****************************
   2          * File Name          : GPIOInit.c
   3          * Author             : Vina Peng,Fortiortech  Appliction Team
   4          * Version            : V1.0
   5          * Date               : 010-Apr-2017
   6          * Description        : This file contains GPIO initial function used for Motor Control.
   7          ***************************************************************************************************
   8          * All Rights Reserved
   9          **************************************************************************************************/
  10          
  11          /* Includes -------------------------------------------------------------------------------------*/
  12          #include <FU68xx_2.h>
  13          #include <Myproject.h>
  14          
  15          /*-------------------------------------------------------------------------------------------------
  16            Function Name :  void GPIO_Default_Init(void)
  17            Description   :  为提高芯片的抗干扰能力，降低芯片功耗，请在具体项目时，将不
             -需要用的GPIO默认都配置为输入上拉。
  18            Input         :  无
  19            Output        :  无
  20          -------------------------------------------------------------------------------------------------*/
  21          //void GPIO_Default_Init(void)//为提高芯片的抗干扰能力，降低芯片功耗，请在具体项�
             -�时，将不需要用的GPIO默认都配置为输入上拉。
  22          //{
  23          //    SetBit(P0_OE, P07);       // config P11 as output,0 as input,1 as output
  24          //    SetBit(P0_PU, P07);  // enable P11 pull up        ,0 as disable,1 as enable       
  25          //    GP07 = 1;
  26          //}


MODULE INFORMATION:   STATIC OVERLAYABLE
   CODE SIZE        =   ----    ----
   CONSTANT SIZE    =   ----    ----
   XDATA SIZE       =   ----    ----
   PDATA SIZE       =   ----    ----
   DATA SIZE        =   ----    ----
   IDATA SIZE       =   ----    ----
   BIT SIZE         =   ----    ----
   EDATA SIZE       =   ----    ----
   HDATA SIZE       =   ----    ----
   XDATA CONST SIZE =   ----    ----
   FAR CONST SIZE   =   ----    ----
END OF MODULE INFORMATION.


C51 COMPILATION COMPLETE.  0 WARNING(S),  0 ERROR(S)
