#

##

##

    礦ision Build Log
    Project:
    C:\Users\Administrator\Desktop\2018年进行的项目\0.MCU项目\00 ！！！程序规范\FU6802_Time4_例程\FU6802_TIM4\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\KeilC51\FOC_Fortior.uvproj
    Project File Date:  09/28/2018

    Output:
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=0 const=0 code=177
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 177 bytes programmed.
    Flash Verify Done: 177 bytes verified OK, CrcVal:0xb574.
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 177 bytes programmed.
    Flash Verify Done: 177 bytes verified OK, CrcVal:0xb574.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=0 const=0 code=177
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 177 bytes programmed.
    Flash Verify Done: 177 bytes verified OK, CrcVal:0x5c4d.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    compiling GPIOInit.c...
    linking...
    Program Size: data=9.0 xdata=0 const=0 code=181
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 181 bytes programmed.
    Flash Verify Done: 181 bytes verified OK, CrcVal:0xb660.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=0 const=0 code=183
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 183 bytes programmed.
    Flash Verify Done: 183 bytes verified OK, CrcVal:0xa7fb.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    *** ERROR L127: UNRESOLVED EXTERNAL SYMBOL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
    *** ERROR L127: UNRESOLVED EXTERNAL SYMBOL
        SYMBOL:  PWMARR
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 1000062H
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMARR
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 1000074H
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 100008BH
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 1000095H
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMARR
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 100009FH
    Program Size: data=9.0 xdata=0 const=0 code=206
    Target not created
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    *** ERROR L127: UNRESOLVED EXTERNAL SYMBOL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
    *** ERROR L127: UNRESOLVED EXTERNAL SYMBOL
        SYMBOL:  PWMARR
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 1000062H
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMARR
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 1000074H
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 100008BH
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMCompare
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 1000095H
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  PWMARR
        MODULE:  .\Output\Interrupt.obj (INTERRUPT)
        ADDRESS: 100009FH
    Program Size: data=9.0 xdata=0 const=0 code=206
    Target not created
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=204
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 204 bytes programmed.
    Flash Verify Done: 204 bytes verified OK, CrcVal:0x0e06.
    Rebuild target 'FU68XX_FOC'
    compiling main.c...
    compiling Interrupt.c...
    compiling TimerInit.c...
    compiling GPIOInit.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=204
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 204 bytes programmed.
    Flash Verify Done: 204 bytes verified OK, CrcVal:0x0e06.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=215
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 215 bytes programmed.
    Flash Verify Done: 215 bytes verified OK, CrcVal:0xa2c9.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=204
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 204 bytes programmed.
    Flash Verify Done: 204 bytes verified OK, CrcVal:0x0e06.
    Rebuild target 'FU68XX_FOC'
    compiling main.c...
    compiling Interrupt.c...
    compiling TimerInit.c...
    compiling GPIOInit.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=204
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 204 bytes programmed.
    Flash Verify Done: 204 bytes verified OK, CrcVal:0x0e06.
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 204 bytes programmed.
    Flash Verify Done: 204 bytes verified OK, CrcVal:0x0e06.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=217
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 217 bytes programmed.
    Flash Verify Done: 217 bytes verified OK, CrcVal:0x2d06.
    Build target 'FU68XX_FOC'
    compiling GPIOInit.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=221
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 221 bytes programmed.
    Flash Verify Done: 221 bytes verified OK, CrcVal:0x7dff.
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 221 bytes programmed.
    Flash Verify Done: 221 bytes verified OK, CrcVal:0x7dff.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=212
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 212 bytes programmed.
    Flash Verify Done: 212 bytes verified OK, CrcVal:0x372f.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=208
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 208 bytes programmed.
    Flash Verify Done: 208 bytes verified OK, CrcVal:0xa279.
    Rebuild target 'FU68XX_FOC'
    compiling main.c...
    compiling Interrupt.c...
    compiling TimerInit.c...
    compiling GPIOInit.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=208
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).
    Load "C:\\Users\\Administrator\\Desktop\\2018年进行的项目\\0.MCU项目\\00 ！！！程序规范\\FU6802_Time4_例程\\FU6802_TIM4\\FU68xx_2_TIM4___输入timer模式___PWM捕获模式\\KeilC51\\Output\\FOC_Fortior"
    device is connecting...
    *** Successful: 1
    *** Successful: Device [00] Find--->SN: ftk&0#{53f56307-
    Flash Erase Done.
    Write Ccfg Parameters Done.
    Flash Write Done: 208 bytes programmed.
    Flash Verify Done: 208 bytes verified OK, CrcVal:0xa279.
    Build target 'FU68XX_FOC'
    compiling Interrupt.c...
    linking...
    Program Size: data=9.0 xdata=4 const=0 code=201
    creating hex file from ".\Output\FOC_Fortior"...
    ".\Output\FOC_Fortior" - 0 Error(s), 0 Warning(s).