C51 COMPILER V9.52.0.0   INTERRUPT                                                         09/28/2018 14:16:58 PAGE 1   


C51 COMPILER V9.52.0.0, COMPILATION OF MODULE INTERRUPT
OBJECT MODULE PLACED IN .\Output\Interrupt.obj
COMPILER INVOKED BY: D:\FortiorTech\Software\Mcu\C51\BIN\C51.EXE ..\User\Source\Application\Interrupt.c LARGE OMF2 WARNI
                    -NGLEVEL(0) BROWSE INCDIR(..\Library\FU68xx_Hardware_Driver\Include;..\User\Include) DEBUG PRINT(.\Listing\Interrupt.lst)
                    - OBJECT(.\Output\Interrupt.obj)

line level    source

   1          /**************************** (C) COPYRIGHT 2017 Fortiortech shenzhen *****************************
   2          * File Name          : Interrupt.c
   3          * Author             : Vina Peng,Fortiortech  Appliction Team
   4          * Version            : V1.0
   5          * Date               : 2017-12-26
   6          * Description        : This file contains all the interrupt function used for Motor Control.
   7          ***************************************************************************************************
   8          * All Rights Reserved
   9          **************************************************************************************************/
  10          
  11          
  12          /* Includes -------------------------------------------------------------------------------------*/
  13          // #include <Interrupt.h>
  14          #include <FU68xx_2.h>
  15          #include <Myproject.h>
  16          #include <Customer_Debug.h>
  17          uint16 xdata spidebug[4] = { 0 };
  18          
  19          /*---------------------------------------------------------------------------*/
  20          /* Name     :   void TIM23_INT(void) interrupt 9
  21          /* Input    :   NO
  22          /* Output   :   NO
  23          /* Description: Capture PWM ，中断优先级第二，高于FOC中断，用于PWM调速
  24          /*---------------------------------------------------------------------------*/
  25          void TIM3_INT(void) interrupt 9
  26          {
  27   1              
  28   1          if(ReadBit(TIM3_CR1, T3IF))
  29   1          {
  30   2              GP07 = ~GP07;
  31   2              ClrBit(TIM3_CR1, T3IF);
  32   2          }
  33   1      }


MODULE INFORMATION:   STATIC OVERLAYABLE
   CODE SIZE        =     18    ----
   CONSTANT SIZE    =   ----    ----
   XDATA SIZE       =      8    ----
   PDATA SIZE       =   ----    ----
   DATA SIZE        =   ----    ----
   IDATA SIZE       =   ----    ----
   BIT SIZE         =   ----    ----
   EDATA SIZE       =   ----    ----
   HDATA SIZE       =   ----    ----
   XDATA CONST SIZE =   ----    ----
   FAR CONST SIZE   =   ----    ----
END OF MODULE INFORMATION.


C51 COMPILATION COMPLETE.  0 WARNING(S),  0 ERROR(S)
