C51 COMPILER V9.52.0.0   INTERRUPT                                                         09/28/2018 15:04:33 PAGE 1   


C51 COMPILER V9.52.0.0, COMPILATION OF MODULE INTERRUPT
OBJECT MODULE PLACED IN .\Output\Interrupt.obj
COMPILER INVOKED BY: D:\FortiorTech\Software\Mcu\C51\BIN\C51.EXE ..\User\Source\Application\Interrupt.c LARGE OMF2 WARNI
                    -NGLEVEL(0) BROWSE INCDIR(..\Library\FU68xx_Hardware_Driver\Include;..\User\Include) DEBUG PRINT(.\Listing\Interrupt.lst)
                    - OBJECT(.\Output\Interrupt.obj)

line level    source

   1          /**************************** (C) COPYRIGHT 2017 Fortiortech shenzhen *****************************
   2          * File Name          : Interrupt.c
   3          * Author             : Vina Peng,Fortiortech  Appliction Team
   4          * Version            : V1.0
   5          * Date               : 2017-12-26
   6          * Description        : This file contains all the interrupt function used for Motor Control.
   7          ***************************************************************************************************
   8          * All Rights Reserved
   9          **************************************************************************************************/
  10          
  11          
  12          /* Includes -------------------------------------------------------------------------------------*/
  13          // #include <Interrupt.h>
  14          #include <FU68xx_2.h>
  15          #include <Myproject.h>
  16          #include <Customer_Debug.h>
  17          uint16 xdata spidebug[4] = { 0 };
  18          
  19          /*---------------------------------------------------------------------------*/
  20          /* Name     :   void TIM23_INT(void) interrupt 9
  21          /* Input    :   NO
  22          /* Output   :   NO
  23          /* Description: Capture PWM ，中断优先级第二，高于FOC中断，用于PWM调速
  24          /*---------------------------------------------------------------------------*/
  25          //void TIM3_INT(void) interrupt 9
  26          //{
  27          //      
  28          //    if(ReadBit(TIM3_CR1, T3IR))
  29          //    {
  30          //        ClrBit(TIM3_CR1, T3IR);
  31          //    }
  32          //    if(ReadBit(TIM3_CR1, T3IP))//周期中断
  33          //    {
  34          //        mcPwmInput.PWMCompare    = TIM3__DR;
  35          //        mcPwmInput.PWMARR        = TIM3__ARR;
  36          //        mcPwmInput.PWMFlag = 1;
  37          
  38          //        ClrBit(TIM3_CR1, T3IP);
  39          //    }
  40          //    if(ReadBit(TIM3_CR1, T3IF))
  41          //    {
  42          //        ClrBit(TIM3_CR1, T3IF);
  43          //    }
  44          //}


MODULE INFORMATION:   STATIC OVERLAYABLE
   CODE SIZE        =   ----    ----
   CONSTANT SIZE    =   ----    ----
   XDATA SIZE       =      8    ----
   PDATA SIZE       =   ----    ----
   DATA SIZE        =   ----    ----
   IDATA SIZE       =   ----    ----
C51 COMPILER V9.52.0.0   INTERRUPT                                                         09/28/2018 15:04:33 PAGE 2   

   BIT SIZE         =   ----    ----
   EDATA SIZE       =   ----    ----
   HDATA SIZE       =   ----    ----
   XDATA CONST SIZE =   ----    ----
   FAR CONST SIZE   =   ----    ----
END OF MODULE INFORMATION.


C51 COMPILATION COMPLETE.  0 WARNING(S),  0 ERROR(S)
