C51 COMPILER V9.52.0.0   FOCCONTROLFUNCTION                                                09/28/2018 10:01:24 PAGE 1   


C51 COMPILER V9.52.0.0, COMPILATION OF MODULE FOCCONTROLFUNCTION
OBJECT MODULE PLACED IN .\Output\FocControlFunction.obj
COMPILER INVOKED BY: C:\Keil\C51\BIN\C51.EXE ..\User\Source\Function\FocControlFunction.c LARGE OMF2 WARNINGLEVEL(0) BRO
                    -WSE INCDIR(..\Library\FU68xx_Hardware_Driver\Include;..\User\Include) DEBUG PRINT(.\Listing\FocControlFunction.lst) OBJE
                    -CT(.\Output\FocControlFunction.obj)

line level    source

   1          /**************************** (C) COPYRIGHT 2017 Fortiortech shenzhen *****************************
   2          * File Name          : FocControl.c
   3          * Author             : Vina Peng,Fortiortech  Appliction Team
   4          * Version            : V1.0
   5          * Date               : 10-Apr-2017
   6          * Description        : This file contains all the foc control function used for motor control.
   7          ***************************************************************************************************
   8          * All Rights Reserved
   9          **************************************************************************************************/
  10          
  11          
  12          /* Includes -------------------------------------------------------------------------------------*/
  13          #include <FU68xx_2.h>
  14          #include <Myproject.h>
  15          #include <FU68xx_2_DMA.h>
  16          #endif
  17          CurrentOffset xdata mcCurOffset;
  18          
  19          /*-------------------------------------------------------------------------------------------------
  20            Function Name :  void MotorControlInit(void)
  21            Description   :  控制变量初始化清零,包括保护参数的初始化、电机状态初始化
  22            Input         :  输入说明（详细）
  23            Output        :  输出说明（详细）
  24          -------------------------------------------------------------------------------------------------*/
  25          void MotorcontrolInit(void)
  26          {
  27   1      
  28   1        /*PWM调速变量*/
  29   1        memset(&mcPwmInput,0, sizeof(PWMINPUTCAL));                            // mcPwmInput变量清零
  30   1        temp32 = 0;
  31   1      }
  32          


MODULE INFORMATION:   STATIC OVERLAYABLE
   CODE SIZE        =     25    ----
   CONSTANT SIZE    =   ----    ----
   XDATA SIZE       =     21    ----
   PDATA SIZE       =   ----    ----
   DATA SIZE        =   ----    ----
   IDATA SIZE       =   ----    ----
   BIT SIZE         =   ----    ----
   EDATA SIZE       =   ----    ----
   HDATA SIZE       =   ----    ----
   XDATA CONST SIZE =   ----    ----
   FAR CONST SIZE   =   ----    ----
END OF MODULE INFORMATION.


C51 COMPILATION COMPLETE.  0 WARNING(S),  0 ERROR(S)
