C51 COMPILER V9.52.0.0   MPU6050                                                           09/21/2018 15:56:35 PAGE 1   


C51 COMPILER V9.52.0.0, COMPILATION OF MODULE MPU6050
OBJECT MODULE PLACED IN .\Output\MPU6050.obj
COMPILER INVOKED BY: F:\keil\C51\BIN\C51.EXE ..\User\Source\Application\MPU6050.c LARGE OMF2 WARNINGLEVEL(0) BROWSE INCD
                    -IR(..\Library\FU68xx_Hardware_Driver\Include;..\User\Include) DEBUG PRINT(.\Listing\MPU6050.lst) OBJECT(.\Output\MPU6050
                    -.obj)

line level    source

   1          #include <FU68xx_2.h>
   2          #include <Myproject.h>
   3          
   4          void MPU6060_Init(void)
   5          {
   6   1              Write_I2C_Byte(SlaveAddress >> 1, PWR_MGMT_1, 0x00);
   7   1              Write_I2C_Byte(SlaveAddress >> 1, SMPLRT_DIV, 0x07);
   8   1              Write_I2C_Byte(SlaveAddress >> 1, CONFIG, 0x06);
   9   1              Write_I2C_Byte(SlaveAddress >> 1, GYRO_CONFIG, 0x18);
  10   1              Write_I2C_Byte(SlaveAddress >> 1, ACCEL_CONFIG, 0x01);
  11   1      }


MODULE INFORMATION:   STATIC OVERLAYABLE
   CODE SIZE        =     45    ----
   CONSTANT SIZE    =   ----    ----
   XDATA SIZE       =   ----    ----
   PDATA SIZE       =   ----    ----
   DATA SIZE        =   ----    ----
   IDATA SIZE       =   ----    ----
   BIT SIZE         =   ----    ----
   EDATA SIZE       =   ----    ----
   HDATA SIZE       =   ----    ----
   XDATA CONST SIZE =   ----    ----
   FAR CONST SIZE   =   ----    ----
END OF MODULE INFORMATION.


C51 COMPILATION COMPLETE.  0 WARNING(S),  0 ERROR(S)
